Sound Design Toolkit 075 Physically informed sound synthesis for everyday sounds

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

Macros | Functions | Variables
SDTCommon.h File Reference

Go to the source code of this file.

## Macros
#define | SDT_ver 075
| SDT version number.
#define | SDT_ver_str "075"
| SDT version string.
#define | SDT_PI 3.141592653589793
| Value of Pi.
#define | SDT_TWOPI 6.283185307179586
| Value of 2 * Pi.
#define | SDT_EULER 2.718281828459045
| Euler number.
#define | SDT_SQRT2 1.4142135623730951
| Square root of 2.
#define | SDT_MACH1 340.29
| Mach 1, speed of sound in air under normal atmospheric conditions (m/s)
#define | SDT_EARTH 9.81
| Earth gravity (N/Kg)
#define | SDT_MICRO 0.000001
| One millionth, small value often used instead of 0 to avoid division errors.
#define | SDT_QUIET 0.00003
| Gain factor roughly corresponding to a -90dB attenuation.

## Functions
void | SDT_setSampleRate (double sampleRate)
| Sets the sample rate. More...
unsigned int | SDT_bitReverse (unsigned int u, unsigned int bits)
| Reverses the bit order of an unsigned integer of given bit length. More...
long | SDT_clip (long x, long min, long max)
| Clips an integer value. Limits the range of an integer value between a given lower bound and upper bound. More...
double | SDT_expRand (double lambda)
| Exponential random number generator. Generates random numbers, following an exponential distribution. More...
double | SDT_fclip (double x, double min, double max)
| Clips a floating point value. Limits the range of a floating point value between a given lower bound and upper bound. More...
double | SDT_frand ()
| Uniform random number generator. Generates random numbers, following a uniform distribution. More...
double | SDT_gravity (double mass)
| Computes earth gravity force. Computes the earth gravity force acting on an object of a given mass. More...
void | SDT_hanning (double *sig, int n)
| Applies a Hanning window to a chunk of samples. Applies a Hanning window to a chunk of samples. More...
void | SDT_haar (double *sig, long n)
| Computes a direct Haar Wavelet Transform of the incoming signal (in place). More...
void | SDT_ihaar (double *sig, long n)
| Computes an inverse Haar Wavelet Transform of the incoming signal (in place). More...
double | SDT_kinetic (double mass, double velocity)
| Computes kinetic energy. Computes the kinetic energy of an object, given its mass and velocity. More...
unsigned int | SDT_nextPow2 (unsigned int u)
| Returns the smallest power of 2 greater or equal than u. More...
double | SDT_normalize (double x, double min, double max)
| Rescales a value of known range into the [0.0, 1.0] interval. Rescales a value of known range into the [0.0, 1.0] interval. More...
void | SDT_normalizeWindow (double *sig, int n)
| Normalizes samples in a window so that their sum is equal to 1. More...
double | SDT_samplesInAir (double length)
| Time needed to travel the given distance at Mach 1. Computes the amount of time, in samples, needed by a sound wave propagating in air to travel a given distance. Particularly useful to set the delay times of comb filters and/or digital waveguides representing hollow cavities. More...
double | SDT_scale (double x, double srcMin, double srcMax, double dstMin, double dstMax, double gamma)
| Rescales a value from a source range to a target range. Rescales a value from a source range to a target range. More...
int | SDT_signum (double x)
| Computes the signum function. Computes the signum function. More...

## Variables
double | SDT_sampleRate
| Sampling frequency (Hz)
double | SDT_timeStep
| Sampling period (s)